{"text_format":"1","workbook":"xlsx","n_sheets":8,"sheets":["SensorLanceType","ThermowellType","TS500_DIN_Cyl","TS500_DIN_tap","TS500_ANSI_NIP","TS500_ANSI_NUN","TWPictures","Language"],"not_rendered":{"charts":0,"images":30,"macros":1,"external_links":0,"defined_names":43,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"SensorLanceType","index":0,"n_rows":8,"n_cols":2,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[null,"Choose Your Temperature Sensor Type:"]

{"sheet":"ThermowellType","index":1,"n_rows":78,"n_cols":16,"rows_kept":78,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[null,"Choose Your Thermowell Type:"]
[]
[]
[]
[]
[null,null,null,"Thread cyl",null,null,"Thread tap",null,null,"Weld-in",null,null,"Flanged",null,null,"Van-Stone"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"DIN"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Straight"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Reduced"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Tapered"]

{"sheet":"TS500_DIN_Cyl","index":2,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
["SITANS TS Temperature Sensor"]
["SITRANS TS500 Build-in 7MC7500*"]
[]
[]
[null,null,null,null,null,null,"7MC7500-*",null,"***"]
[null,null,null,null,null,null,"Tread type"]
[null,null,null,null,null,null,"G1/2\"","C"]
[null,null,null,null,null,null,"M14x1,5","T"]
[null,null,null,null,null,null,"M18x1,5","U"]
[null,null,null,null,null,null,"M20x1,5","V"]
[null,null,null,null,null,null,"Extension X"]
[null,null,null,null,null,null,"X=65 mm",null,null,1]
[null,null,null,null,null,null,"X=139 mm",null,null,2]
[null,null,null,null,null,null,"X=149 mm",null,null,3]
[null,null,null,null,null,null,"X= customer spec.",null,null,9,"N*D"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"Insertion length","UTS500=",289,"mm          or",{"$f":"UTS_TS500_DIN_Cyl/25.4","v":11.377952755905513},"inch"]
[]
[]
[]
["Thermowell"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"Length","L=",290,"mm          or",null,"inch"]
[]
[null,null,null,null,null,"Insertion length","UTW=",200,"mm          or",null,"inch"]
[]
[null,null,null,null,null,"Head length","X1=",90,"mm          or",null,"inch"]

{"sheet":"TS500_DIN_tap","index":3,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
["SITANS TS Temperature Sensor"]
["SITRANS TS500 Build-in 7MC7500*"]
[]
[]
[null,null,null,null,null,null,"7MC7500-*",null,"***"]
[null,null,null,null,null,null,"Tread type"]
[null,null,null,null,null,null,"1/2\" NPT","J"]
[]
[]
[]
[null,null,null,null,null,null,"Extension X"]
[null,null,null,null,null,null,"X=65 mm",null,null,1]
[null,null,null,null,null,null,"X=139 mm",null,null,2]
[null,null,null,null,null,null,"X=149 mm",null,null,3]
[null,null,null,null,null,null,"X= customer spec.",null,null,9,"N*D"]
[]
[]
[null,null,null,"Please note the mechanical tolerance of NPT thread (ca. 3 mm)!"]
[null,null,null,null,"Preffered solution: compensation with PTFE-tape"]
[null,null,null,null,"Alternatively: shorter insert length"]
[]
[]
[null,null,null,null,"Insertion length with tape",null,"UTS500=",287,"mm          or",{"$f":"PTFE_TS500_DIN_tap/25.4","v":11.299212598425198},"inch"]
[]
[null,null,null,null,"Insertion length without tape",null,"UTS500=",284,"mm          or",{"$f":"UTS_TS500_DIN_tap/25.4","v":11.181102362204726},"inch"]
[]
[]
["Thermowell"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"Length","L=",290,"mm          or",null,"inch"]
[]
[null,null,null,null,null,"Insertion length","UTW=",200,"mm          or",null,"inch"]
[]
[null,null,null,null,null,"Head length","X1=",90,"mm          or",null,"inch"]

{"sheet":"TS500_ANSI_NIP","index":4,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
["SITANS TS Temperature Sensor"]
["SITRANS TS500 Build-in 7MC7500*"]
[]
[]
[null,null,null,null,null,null,"7MC7500-*",null,"***"]
[null,null,null,null,null,null,"Tread type"]
[null,null,null,null,null,null,"1/2\" NPT","J"]
[]
[]
[]
[null,null,null,null,null,null,"Extension X"]
[null,null,null,null,null,null,"X=74 mm (2.91 inch)  -  NIP",null,null,6]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"Insertion length","UTS500=",290,"mm           or",{"$f":"UTS_TS500_ANSI_NIP/25.4","v":11.41732283464567},"inch"]
[]
[]
[]
["Thermowell"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"Length","L=",290,"mm           or",null,"inch"]
[]
[null,null,null,null,null,"Insertion length","UTW=",200,"mm           or",null,"inch"]
[]
[null,null,null,null,null,"Head length","X1=",90,"mm           or",null,"inch"]

{"sheet":"TS500_ANSI_NUN","index":5,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
["SITANS TS Temperature Sensor"]
["SITRANS TS500 Build-in 7MC7500*"]
[]
[]
[null,null,null,null,null,null,"7MC7500-*",null,"***"]
[null,null,null,null,null,null,"Tread type"]
[null,null,null,null,null,null,"1/2\" NPT","J"]
[]
[]
[]
[null,null,null,null,null,null,"Extension X"]
[null,null,null,null,null,null,"X=150 mm (5.91 inch)  -  NUN",null,null,8]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"Insertion length","UTS500=",290,"mm           or",{"$f":"UTS_TS500_ANSI_NUN/25.4","v":11.41732283464567},"inch"]
[]
[]
[]
["Thermowell"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"Length","L=",290,"mm           or",null,"inch"]
[]
[null,null,null,null,null,"Insertion length","UTW=",200,"mm           or",null,"inch"]
[]
[null,null,null,null,null,"Head length","X1=",90,"mm           or",null,"inch"]

{"sheet":"TWPictures","index":6,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Language","index":7,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["German","English"]